23-11-25

To improve the deviation on narrow band

2023-9-25

1、to solve the issue that when MD-619 transmit, Motorola radio receive but no tone

Press side key under PTT to power on and hold on, open the programming software and choose the correct comm. port, and click Shift + Ctrl + Alt + I, the updating window will appear, then choose the firmware and click download, the red circle beside comm. port will turn green and it starts to update



