Channel - > DMR Digital Channel -TDMA Adaption

TDMA adaption mode, the Radio can randomly select the available time slot emissions, rather than fixed a time slot. After TDMA adaption mode is enabled, in any of the two time slots, the language call and data transmission can be carried out in the through mode.

Check: Allows to enable TDMA adaption mode on the current channel.

Uncheck： Prohibit TDMA adaption mode on the current channel.

Default:

Uncheck

Note:

-Only hand-held and mobile radio supports this feature.