DMR Settings -Basic settings -Call Hang Time

# Call Hang Time

Sets the duration the radio keeps the digital communication at the current digital channel after the end of a call transmission. During this time, all members of the call that the channel is reserved can still transmit.

This is to avoid setting up the different channel again each time the user presses the PTT to transmit, and produces smoother

Range:

0~10 sec

Step:

1 sec

Default:

0 sec

Note:

-This feature is not effective when the value is set to 0 sec

-This feature is supported in Digital mode only.