Channel- Mixed Channel-Digital Available Channel

# Digital Available Channel

Shows all alternative digital channels associated by the setting of Digital Channel Type. The selected digital channel becomes the digital channel parameter of the current mixed channel. This setting is effective on the programmed channel only.

Options:

DPMR digital channel 1~509 or DMR digital channel 1~509

Default:

DMR digital channel 1

Note:

If the frequencies of digital channel and analog channel are inconsistent, the analog channel frequency would be the base frequency of the mixed channel.