DPMR Settings -Basic Settings -Confirm Response Delay Time

# Confirm Response Delay Time

This duration is a string of bits added in front of a response(ACK) frame before transmitting. This preamble prolongs the response frame in order to reduce the chances of the response frame being missed by the receiving radio. This feature sets the duration of the preamble for the confirmed response.

Range:

None

40 ms

80 ms

160 ms

320 ms

Default:

80 ms