Channel-DPMR Digital Channel -Basic Encryption key

# Basic Encryption key

The Basic encryption key is used to scramble and unscramble voice calls and data transmissions on privacy-enabled channels. Receiving radio(s) must have the same Basic encryption key as the transmitting radio in order to unscramble the privacy-enabled voice call or to receive the privacy-enabled data transmission.

Range:

0~65535

Default:

0

Note:

-This feature is disabled if Encryption feature is unchecked.