Channel-DMR Digital Channel -Admit Criteria

# Admit Criteria

Determines when voice or data is allowed to be transmitted on the channel. This is used to prevent a radio from transmitting on channels that are already being used.

Options:

Always: The radio will always transmit when the Push-to-Talk (PTT) key is pressed

Channel Free: The radio will check for an idle channel prior to allowing a transmission.

CC Free: The radio will check if the specified Color Code is not in use prior to allowing transmission (except for Group Calls that are already in progress).

Default:

Always

Note:

-The RX Only feature must be disabled