Scan List -Tx Designated Channel

Tx Designated Channel

Defines the channel on which the radio will transmit if the user presses the PTT key while the radio is scanning. If the Talkback option is disabled, this feature also defines the channel where the radio will transmit if the user presses the PTT when the radio has stopped scanning to unmute to an eligible scan list member.

Options:

Current Channel: The channel indicated by the channel selector.

Last Active Channel: The last channel where the radio in scan mode stopped and unmuted to receive audio.

Default:

Current Channel