Channel-DMR Digital Channel -Tx CC

# Tx CC

A color code is used to identify a system. Different color codes are used to identify different system. Radios in a system should have the same color code to communicate each other. Radios will ignore any channel activity not containing the matching color code for that system. A radio is able to scan across channels with different codes for roaming between multiple systems.

Range:

0~15

Step:

1

Default:

1

Note:

-This feature is applicable in Digital mode only.