Channel-Mixed Channel-Mixed Channel Hang Time

# Mixed Channel Hang Time

Sets the duration the radio keeps the digital communication at the mixed channel after the end of a digital call transmission. During this time, all members of the call that the channel is reserved can still transmit. This is to avoid setting up the different channel mode again each time the user presses the PTT to transmit, and produces smoother

Range:

0~10 sec

Step:

1 sec

Default:

1 sec