Channel- Analog Channel -Rx Squelch Level

# Rx Squelch Level

This feature adjusts the squelch threshold of an incoming transmission. When the user increases the squelch level, the radio can receive a stronger signal and filters incoming signals that are not strong enough to produce a clear transmission, thereby eliminating unwanted noise.

Options:

0: Squelch normally open

1,2,3,4

Default:

3: Open