Channel-Analog Channel - Tx Sub-audio Code

# Tx Sub-audio Code

Sets the designated digital code transmitted on a CTCSS/DCS coded transmission for the current channel. When receiver that is set to respond to the transmitted tone sequences receives the correct tone sequence, it indicates user has been called and unmutes radio, so that activity on the channel can be heard. Others will remain muted.

Range:

023~754

Default:

023

Note:

-This feature is supported in Analog mode only.

-The RX Only feature must be disabled

-This feature is applicable when setting Tx Squelch Type to CTCSS/DCS code or Reverse CTCSS/DCS code