DMR Settings -Basic settings -OACSU Retry Limit

# OACSU Retry Limit

Sets the number of retry Off Air Call Setup(OACSU) that the transmitting radio attempts a presence check of the receiving radio. When the transmitting radio failed to receive the response from the receiving radio and OACSU Waiting Timer expires, it retries to initiate the same individual call. Even after retrying to initiate the same individual call as many as times specified by this feature, if the transmitting radio failed to receive the response from the receiving radio, this individual call would be considered as the failure of setup.

Range:

1~10

Step:

1

Default:

2