Channel-Analog Channel -Scan List

# Scan List

This feature is linked to an existing scan list of DMR digital channel. A radio scans for voice activity by cycling through the channel sequence specified in the scan list for the current channel. A radio can support up to 10 scan lists, with a maximum of 16 members in a list. Each scan list supports a mixture of both analog and digital entries.

Options:

None: Do not initiate scanning on the current channel.

Scan List 1~Maximum number of scan lists

Default:

None