Channel-DMR Digital Channel -Channel Alias

# Channel Alias

The user can set an alias for the channel. The user may enter up to a maximum of 16 characters. Valid characters are alphanumeric, spaces and special characters. Refer to the below note section.

Note:

-If the alias length exceeds the maximum length that can be displayed, a radio will cut off some excess automatically, in general, the maximum length of the alias at each model is as following :

Hand-held: 15 digits or 10 to 16 alphabet characters or 8 Chinese characters.

Mobile: 13 to 16 digits or 8 to 16 alphabet characters or 7 Chinese characters

Repeater: 16 digits or 10 to 16 alphabet characters or 8 Chinese characters.