Channel - > DMR Digital Channel-TX Interrupt

This function allows interrogators that support transmission interruption to be interrupted during voice transmission. After the intercom is interrupted, voice, emergency call or data transmission can continue. To configure the radio to support transmission interruption, refer to the Preset KEY settings for the TX interrupt function.

Options:

Check: Enable TX interrupt function.

Uncheck : Disable TX interrupt function.

Default:

Uncheck

Note:

-The RX Only feature must be disabled .