Channel-DPMR Digital Channel -Copy

# Copy

Copy the Receive Frequency to the Transmit Frequency.

For an Analog channel, this feature also copies all the Receive parameters, i.e. features inside the RX box such as the Frequency (MHz), Voice Type and Sub-audio to the Transmit side.

For a Digital channel, the RX box has only the Receive Frequency (MHz) feature, therefore only this is copied to the Transmit side.

Note:

-This button is unavailable when RX Only feature is enabled.