Channel-DMR Digital Channel -Time-Out Timer(TOT)

# Time-Out Timer(TOT)

The Time-Out Timer(TOT) is the duration that the radio can continuously transmit before a transmission is automatically terminated. This feature is used to ensure the channel is not monopolized by any one radio.

Options:

No Limitation

30 sec

60 sec

90 sec

120 sec

Default:

Infinity

Note:

-This feature is applicable to hand-held and mobile radio only

-Time-out timer for this channel will be disabled if the Infinity(?) option is selected.

-The RX Only feature must be disabled