Channel-DMR Digital Channel -Slot

# Slot

DMR utilizes digital Time Division Multiple Access (TDMA) technology to divide a 12.5kHz channel into two alternating time slots, with each carrying an individual call when operating in Repeater mode. As a result, both the assigned frequency and the assigned time slot must be specified in order to completely describe a digital repeater channel. Radios or Groups that need to talk together must be assigned to the same frequency and time slot.

Options:

Slot 1: When operating in Repeater mode, slot 1 is always used for transmission and reception. When operating in Talkaround mode, this feature is not applicable because a radio will always hear another radio transmitting.

Slot 2: When operating in Repeater mode, slot 2 is always used for transmission and reception. When operating in Talkaround mode, this feature is not applicable because a radio will always hear another radio transmitting.

Default:

Slot 1

Note:

-This feature is supported in Digital mode only.