Channel- Analog Channel -Rx Squelch Type

# Rx Squelch Type

Sets the type of decoding needed for the radio to receive a call on the channel. This feature allows for more privacy on a frequency.

Options:

Voice Only: Do not set CTCSS/DCS Tone

CTCSS/DCS: Set the designated frequency received when CTCSS/DCS coded transmission is received on the channel.

CTCSS/DCS code: Set the designated digital code received when CTCSS/DCS coded transmission is received on the channel.

Reverse CTCSS/DCS code: Set the designated reverse digital code received when CTCSS/DCS coded transmission is received on the channel.