Channel-DMR Digital Channel -TDMA Direct Mode

# TDMA Direct Mode

Sets the operation of TDMA direct mode. When operating in TDMA direct mode, SDI(Source Dynamic Identifier) level of the radio is used to appoint one radio in the wide area system as the wide area timing leader.

Options:

Disable: Disable TDMA direct mode operation

SDI Level 1: The radio doesn't take a role of correcting channel slot timing

SDI Level 2: The radio is appointed as a channel slot timing correction leader but can accept another higher level leader

SDI Level 3: The radio is appointed as a channel slot timing correction leader in priority and sets the channel slot timing

Default:

Disable

Note:

-This feature is supported in Digital mode only.