Channel-DMR Digital Channel -TOT Rekey Delay

# TOT Rekey Delay

Sets the amount of time that the radio waits on a channel after the Time-Out Timer(TOT) expires (which stops the radio transmission) before allowing the user to transmit again.

Range:

0~10 sec

Step:

1 sec

Default:

0 sec

Note:

-This feature is available when the TOT is not set to Infinity (?).

-The RX Only feature must be disabled