Channel-Analog Channel -Tx Squelch Type

# Tx Squelch Type

Sets the type of encoding needed for the radio to send a call on the channel. This feature allows for more privacy on a frequency.

Options:

Voice Only: Do not set CTCSS/DCS Tone

CTCSS/DCS: Set the designated frequency encoded into the transmitted signal for this channel

CTCSS/DCS code: Set the code representing a specific tone. This tone is encoded into transmissions on this channel.

Reverse CTCSS/DCS code: Set the code representing a specific tone. The reverse tone is encoded into transmissions on this channel.

Note:

-The RX Only feature must be disabled