Channel- Analog Channel -Admit Criteria

# Admit Criteria

Determines when voice is allowed to be transmitted on the channel. This is used to prevent a radio from transmitting on channels that are already being used.

Options:

Always: The radio will always transmit when the Push-to-Talk (PTT) key is pressed

Channel Free: The radio will check for an idle channel prior to allowing a transmission.

CTCSS/DCS Match: The radio will check if the specified tone is matched prior to allowing transmission.

CTCSS/DCS Not Match: The radio will check if the specified tone is not matched prior to allowing transmission.

Default:

Always

Note:

-The RX Only feature must be disabled