Basic Settings -Buttons -Function key

# Function key

The user can select the function of 7 programmable function keys.

Key-1, key-3, key-4, key-5, key-6, key-7 and key-8 can be programmed anyone out of the following options.

Options:

None: Not associated with any function for the key, pressing this key is not effective.

SOS: Initiate an emergency alarm which is a typical function keys associated with.

VOX On/Off: Toggle VOX on or off

High/Low Power: Toggle transmit power level between high and low

Squelch: Toggle squelch level between tight and open

Zone Selection: Allows selection from a list of zones

Remote Check: Determines if a radio is active in a system

Scan On/Off: Toggle scan on or off

Quick Call 1: Directly initiates a predefined Quick Call 1

Quick Call 2: Directly initiates a predefined Quick Call 2

Quick Call 3: Directly initiates a predefined Quick Call 3

Quick Call 4: Directly initiates a predefined Quick Call 4

Quick Call 5: Directly initiates a predefined Quick Call 5

TX Interrupt: Press this button to interrupt an ongoing voice call on the current channel for a new call or data service. When using the transmit interruption function, it is necessary to enable the TX Interrupt function in both the interrupt and the interrupted side.

Default:

None.

Note:

-Key-2 is dedicated as PTT call function and cannot be programmed.