Channel-Analog Channel -Tail Degree

# Tail Degree

CTCSS sends the tone code when Push-to-Talk (PTT) button is pressed. On PTT dekey, the tone signal is stopped, and CTCSS 'reverse burst' is generated and sent to indicate the end of the transmission to the receiving radio. This sub-audible code causes the receiving radio to mute its speaker before the loss of a carrier is detected to eliminate unwanted noise (squelch tail).

Options:

120 degree: 120 degree reverse burst sequence is transmitted at the end of a transmission

180 degree: 180 degree reverse burst sequence is transmitted at the end of a transmission

Default:

180 degree