
[ChText]                                  
100=CH
101=RX Freq
102=TxRreq
103=DEC
104=ENC
105=W/N
106=TX Power
107=Busy
108=Scan Add
109=Set DCS
110=Compander
111=Scramble
112=PTTID
113=Special subsonic
114=Signaling Group
115= Retain 
116= Spe Rx
117=Special DATA

11400=1                    
11401=2
11402=3
11403=4
11404=5
11405=6
11406=7
11407=8
11408=201810                      
11500=OFF                       
11501=A
11502=B
11503=201810
                                    
11600=OFF
11601=ON
11602=201810    


[FreqModeText]         
Text=Freq Mode
0=RxFreq
1=TxRreq
2=DEC
3=ENC
4=W/N
5=TX Power
6=Busy
7=scrambling
8=Compander
9=Scramble
10=PTTID
11=Special subsonic
12=frequency step
13=Signaling Group            
14=message code               
15=Retain               
16=Work Mode

160000=Frequency mode
160001=Channel number
160002=Channel name
160003=Frequency+channel
160004=201810



[Information]
IDS_WINDOWNAME=KST U88 Software
IDS_SoftwareVersion = KST U88 Software Ver1.0             
IDC_Company=   all right reserved 2020 


[KEYFUNDISP]                                                            
KEYSETTXT = Key Set                                                  
KEY1SHORT = KEY1£¨Short£©
KEY1LONG  = KEY1£¨long£©
KEY2SHORT = KEY2£¨Short£©
KEY2LONG  = KEY2£¨long£©

[SetKey1Short]        
0=OFF
1=monitoring
2=High / low power
3=Scanning switch
4=Local alarm
5=Remote alarm
6 = channel broadcast
7 = power prompt


[SetKey1Long]        
0=OFF
1=monitoring
2=High / low power
3=Scanning switch
4=Local alarm
5=Remote alarm
6 = channel broadcast
7 = power prompt


[SetKey2Short]       
0=OFF
1=monitoring
2=High / low power
3=Scanning switch
4=Local alarm
5=Remote alarm
6 = channel broadcast
7 = power prompt


[SetKey2Long]         
0=OFF
1=monitoring
2=High / low power
3=Scanning switch
4=Local alarm
5=Remote alarm
6 = channel broadcast
7 = power prompt


[FUNString]
FunctionSet=function set
1300 = Squelch Level
1301=Tx Tot(S)           
1302=Tx warning(S)                
1303=Language selection              
130300=OFF
130301=Chinese
130302=English
130303=201810                                                    
1304=backlight time(S)     
130400=OFF
130401 = 5S
130402 = 10S
130403 = 15S
130404 = 20S
130405 = 25S
130406 = 30S
130407 = 35S
130408 = 40S
130409 = 45S
130410 = 50S
130411 = 55S
130412 = 60S
130413 = 202005        
1305=saving level                 
130500=Ferq  Test
130501=continuity
130502=201810
1306=Automatic keyboard lock(S)
1307=Sound control level
1308=Voice controlled delay shutdown        
130800=0.5S
130801=1S
130802=1.5S
130803=2S
130804=2.5S
130805=3S
130806=201810
1309=Scanning mode          
130900=order
130901=first
130902=201810
1310=Priority channel
1311=Backlight        
131100=gules
131101=blue
131102=orange
131103=201810
1312=Receive backlight
131200=gules
131201=blue
131202=orange
131203=201810
1313=Wait for backlight
131300=gules
131301=blue
131302=orange
131303=201810
1314=Repeater tail cancellation(MS)
1315=Relay tail detection(MS)
1316=Boot display
131600=Full screen
131601=greetings
131602=Clear screen
131603=201810
1317=PTTLaunch delay(S)
131700=OFF
131701=0.2
131702=0.4
131703=0.6
131704=0.8
131705=1
131706=1.2
131707=1.4
131708=1.6
131709=1.8
131710=2
131711=201810
1318=KeepA
131800=0
131801=1
131802=2
131803=3
131804=4
131805=201810
1318=KeepA
1319=Signalling side tone
131900=OFF
131901=Key
131902=Identity code
131903=Key+Identity code
131904=201810
1320=Radio band selection
132000=65-87M
132001=76-108M
132002=87-108M
132003=96-108M
132004=201810

1350=power saving
1351=Sound control switch
1352=Elimination of emission tail sounds
1353=End of launch tone
1354=Hint
1355=Keytone
1356=Keep1
1357=Keep2






[SignalingSetText]
Title = Signaling setting
0=programming
1=Code
2=Signaling duration(MS)
3=Signaling code interruption time(MS)
4=Group number
5=Local ID
6=Remote halo code
7=Remote death code



[Softwarelanguage]
LANG=Language selection
0= English
1= Chinese


[RadioString]
RadioFreq=Radio frequency

[String]
IDS_WIDE=Wide
IDS_NARROW=Narrow

IDS_OFF=OFF
IDS_ON=ON

IDS_HIGH=High
IDS_LOW=Low

IDS_YES=ON
IDS_NO=OFF

IDS_OPEN=ON
IDS_CLOSE=OFF

IDS_CARRIER=Carrier
IDS_QTDQT=QT/DQT

IDS_START=ON
IDS_END=   END
IDS_BOTH=both

IDS_Wirecom=Write frequency
IDS_Readcom=Read frequency
IDS_modifycom= Batch Write

[Password]
IDS_INPassword = Please input password
IDS_UsedPassword =Password
IDS_NewPassword = new Password
IDS_UPPassword = Display password
IDS_NewPassEnd = Confirm new password
IDC_NEWSETSW = Set new Password

[ModelInfo]                            
0=type selection
Fontname=Arial
FontSize=14                             


[Resource]
1=OK
2=Cancel
100=Communication Port
1000=Reading data from radio...
1001=Writing data to radio...
1002=Read data fail!
1003=Write data fail!
1004=Read data succ!
1005=Write data succ!
1006=Cannot connect the radio!
1007=No valid communication port was found.
1008=Mistake Model!
1009=Data error!
1010=Channel frequency error!
1011=All data will be cleared!
1012=Wrong file type!
1013=File corruption!
1014=Initialization of data packet damage. Please set the function item!
1015=The signaling code is incorrect. There can not be any (0~9, A, B, C, D, *, *) characters. Please re-enter!
1016=Input password is inconsistent twice, please try again!


[MenuText]
Menu_File=File(&F)
ID_FILE_NEW=New(&N)
ID_FILE_OPEN=Open(&O)
ID_FILE_SAVE=Save(&S)
ID_FILE_SAVE_AS=Save_As(&A)...
ID_FILE_PRINT=Print(&P)

Menu_File_Print_Preview=Print_Preview(&V)
Menu_File_Print_Setup=Print_Setup(&R)...
ID_APP_EXIT=Exit(&X)


Menu_Program=Program(&P)
ID_ComWrite=Write Program(&W) 
ID_ComRead=Read Program(&R)  
ID_MENUSETPASS=Batch Write(&T)


Menu_Function =Function(&S)
ID_ModelInfo=ModelInfo(&V)
ID_KEYSET=Key Set(&K)
ID_MENUFUN=Function Set(&M)
ID_FerqMode=Freq Mode(&Q)
ID_DTMFSET=DTMF Set(&T)
ID_Radio=Radio Freq(&B)



Menu_Setting=Set(&S)
ID_ChoiceCOM=Serial port(&O)
ID_LANGUAGE=Language selection(&L)

Menu_Help_Help=Help(&H)
ID_APP_ABOUT=About(&A)...
