
**M7 firmware upgrade instruction**

1. Turn off the the power of M7 first, then press and hold "PTT + Side Key 1" and turning on the power to enter download mode.

2. Plug in the programming cable.



3. Select the correct COM Port in the download tool, then click "Path" to choose the firmware to upgrade.

* 

4. After the upgrade is successful, restart (turning on the power of) the M7.