DPMR Settings -Basic Settings -Message Retry Limit

# Message Retry Limit

Sets the number of retry to send an individual message. When the transmitting radio failed to receive the confirmation from the receiving radio and Message Waiting Timer expires, it retries to send the same individual message. Even after retrying to send the same individual message as many as times specified by this feature, if the transmitting radio failed to receive the confirmation from the receiving radio, this individual message would be considered as the failure of sending.

Range:

1~10

Step:

1

Default:

2