Channel-Mixed Channel

# Mixed Channel

This channel provides Mixed communications services based on the combination of analog FM signal and Digital( DPMR/DMR) signal. User can add mixed channels and delete these channels, but at least a mixed channel should be in the channel list. If the frequencies of digital channel and analog channel are inconsistent, the analog channel frequency would be the base frequency of the mixed channel.

The user can set the following parameters:

- Channel Alias
- Digital Channel Type
- Digital Available Channel
- Analog Available Channel
- Mixed Channel Hang Time
- Mixed Channel Tx Mode