DMR Settings -DMR Contacts -Call Type

# Call Type

Configures one of the following call types;

Options:

Individual call: a call from an individual radio to another individual radio.

Group call: a call from an individual radio to a group of radio.

All call: A one-way call from an individual radio to every radio on that channel. All call do not communicate across different timeslots or channels within the system. The ability to initiate an All call is only programmed into radios that are used in supervisory roles. All other radios monitor All call transmissions by default. This feature is very useful when a supervisor needs to communicate with all users on a logical channel, rather than just a particular group or individual.

Note:

-It allows to configure All call only by selecting All call type.